Next: General Usage, Previous: Requirements, Up: Top

## Installation

### Windows

1. Create a directory on the hard drive to store kat5200 files.
2. Open the archive and extract the files to the directory you created in step 1

### *nix

For *nix versions, you must have zlib ,libSDL, libSDL_image, and libguichan already installed! For Debian perform the following:

1. Save the package to a temporary directory on the hard drive
2. dpkg -i kat5200*.deb (must be root)

For distributions that use RedHat's package manager use the following command

1. rpm -Uvh kat5200*.i386.rpm

For other distributions you can use the alien command to convert the package to the desired format. Refer to your distribution's documentation for how to install the package.

### Updates

From version 0.2, when updating, all that is needed is the executable. The configuration and cart files will be automatically updated.